

## Omega2 First Setup For Smart Meter System

1. Connect to omega wifi ( ssid e.g : Omega-XXXX) , WiFi password : 12345678




1. Open browser and write url <omega-wifi>.local . for example: [http://omega-725b.local/](http://omega-3bf3.local/)



Note : it by default add /OnionOS/ , so you do not need to write it.





1. Follow the startup steps and **connect to the home WiFi network**.
   1. Login to omega2 using account data:
      1. Username: root
      2. Password: onioneer




* 1. Connect to WiFi network (WiFi networks list will be displayed) , then enter wifi network password when required




* 1. System update will be checked ,then click Continue , then click Enter OnionOS , Finish




1. After that the main desktop for omega will be displayed.





1. Click on Terminal , then a black window will be displayed ,
   1. enter login : root
   2. Password : onioneer







1. In Terminal , write these commands one by one:

* wget <http://89.147.133.137/medc/update/install.sh>
* chmod +x install.sh
* ./install.sh





1. Finish